* ~~get hardware programmer~~
* ~~get programmer software~~
* ~~get driver programmer~~
* ~~install driver program~~
  + ~~PIC16F883 - missing?~~
  + ~~"read" to see current driver~~
  + ~~"write" to install new driver~~
* get chatpad
* install chatpad -> arduino interface library
* dissasemble chatpad
  + t6 screwdriver